INSTRUCTION FOR HOW TO INSTALL SCANNER UNDER WINDOW XP

FOR USB MODEL
1.	INSTALL THE DRIVER FIRST BEFORE CONNECTING THE SCANNER. (CD OR DRIVER DOWNLOADS FROM THE WEB SITE).
2.	RESTART THE COMPUTER AND CONNECT THE SCANNER TO THE PC.
3.	AFTER THE COMPUTER RESTART YOU WILL SEE THIS MESSAGE. PLEASE CHOOSE (INSTALL FROM A LIST…..) AND PRESS NEXT. (See: Picture 1)

Picture 1
4.	AFTER PRESSING NEXT YOU WILL SEE THIS MESSAGE. PLEASE CHOOSE (INCLUDE THIS LOCATION IN SEARCH) AND YOU CAN BROWSE TO THE FOLDER WERE YOU HAVE THE SCANNER DRIVER (CD OR DOWNLOAD FILE FOLDER). AND PRESS NEXT. (See: Picture 2 and Picture 3)

Picture 3

Picture 2

5.	AFTER PRESSING OK YOU WILL SEE THIS MESSAGE. PLEASE LOOK AT THE LOCATION AND CHOOSE THE ONE WERE YOUR DRIVER IS LOCATED. (See: Picture 4)

Picture 4

6.	AFTER PRESSING NEXT THE COMPUTER WILL SEARCH FOR THE SCANNER SOFTWARE AND THEN YOU WILL SEE THIS MESSAGE AND JUST PRESS (CONTINUE ANYWAY). AND YOU COMPUTER WILL START TO INSTALL THE DRIVER. (See: Picture 5、Picture 6 and Picture 7)

Picture 5

Picture 6

Picture 7
7.	AFTER THE INSTALLATION IS COMPLY PRESS FINISH AND GO TO START > ALL PROGRAMS > GENIUS COLORPAGE….. > AND CLICK ON KYESCAN, IF YOU SEE THE SMALL SCANNER ICON ON BOTTOM LEFT THEN INSTALLATION IS COMPLY.  (See: Picture 8)

Picture 8